PURPOSE & Description

The purpose of this SOP is to delineate the minimum standards for the use of cardiotoxin when administered to rodents by injection. Cardiotoxin, sourced from *Naja spp*, is used in mice to create a temporary and reproducible acute injury. The LD 50 for cardiotoxin in mice is 2mg/kg toxin/venom intraperitoneal injection.

Scope

This SOP applies to the Principal Investigator (PI) and their laboratory staff.

This SOP applies to the administration of cardiotoxin into animals; once injected into the animal cardiotoxin no longer poses a hazard.

Responsibilities

PIs are responsible for training of their laboratory staff and continued participation in following safety guidelines.

Definitions

* **Clear time** – The period of time required to allow for excretion of a hazardous chemical before standard handling practices can be used.
* **Safety-engineered sharps** –a non-needle sharp or needle device with a built-in safety feature or mechanisms that effectively reduces the risk of an exposure incident. More information on safety engineered sharps can be found here: [[UF EHS Safety-Engineered Sharps Fact Sheet](https://webfiles.ehs.ufl.edu/Safety_Eng_Sharps.pdf#:~:text=What%20is%20a%20safety-engineered%20sharp%3F%20The%20U.S.%20Occupational,effectively%20reduces%20the%20risk%20of%20an%20exposure%20incident.%E2%80%9D)](https://webfiles.ehs.ufl.edu/Safety_Eng_Sharps.pdf#:~:text=What%20is%20a%20safety-engineered%20sharp%3F%20The%20U.S.%20Occupational,effectively%20reduces%20the%20risk%20of%20an%20exposure%20incident.%E2%80%9D).

Hazard Identification & Control Measures

**Potential Hazards**

* **Physical Hazards**
  + Needlestick

**Engineering Controls / Administrative Controls**

* Use of an Animal Transfer Station (ATS) or higher engineering control such as a Biosafety Cabinet (BSC) or Chemical Fume Hood (CFH) is required for agent administration
* Syringes used for injection should comply with the details outlined in [UF EHS Safety-Engineered Sharps Fact Sheet](https://webfiles.ehs.ufl.edu/Safety_Eng_Sharps.pdf#:~:text=What%20is%20a%20safety-engineered%20sharp%3F%20The%20U.S.%20Occupational,effectively%20reduces%20the%20risk%20of%20an%20exposure%20incident.%E2%80%9D).
* Rodents should be appropriately restrained prior to administration, as described in the approved Animal Use Protocol (AUP).
* Gloves should be changed frequently, at a minimum when contaminated with cardiotoxin or torn, and before handling animals in other experimental groups.
* Hands and arms should be washed with soap and water upon completion of procedure.

**Personal Protective Equipment (PPE)**

* Appropriate lab attire including skin protection, closed shoes, and eye protection.
* Long-sleeve gown or long-sleeve dedicated lab coat
* Gloves

Procedure

* Prior to working with chemical hazards in rodents, all work must be described in an approved AUP.

Special Handling and Storage Requirements

* Cardiotoxin could be shed into the bedding; however, once injected into the animal cardiotoxin no longer poses a hazard and may be treated as regular waste.
* Cardiotoxin storage and transport containers should be shatter-resistant, rigid, shock-resistant, leak-proof, and made of a non-reactive material which can be easily cleaned and decontaminated in the event of a leak.
* Personal protective equipment as described above must be worn when handling cardiotoxin, in addition to any PPE requirements of the animal room. Hands and arms should be washed with soap and water after removing PPE.
* Needles and sharps used with cardiotoxin must be disposed of immediately in a sharps container. Do not reuse, bend, or recap needles. Safety-engineered sharps should be used whenever possible.
* An approved solution must be used for decontamination of equipment and areas exposed to cardiotoxin (e.g. Peroxigard).

Waste Disposal Procedures

* Contaminated and/or potentially contaminated laboratory PPE and laboratory consumables are disposed of as regular waste.
* Contaminated and/or potentially contaminated bedding and PPE originating within the animal facility are disposed of as regular waste.
* Rodents euthanized or found dead are disposed of following standard procedures and require no additional handling procedures.

Emergency Response (Spill & Accident Procedures)

**Spills**

* If a small spill occurs, clean up with an approved solution (e.g. Peroxigard). Collect spilled material and clean up material into appropriately labeled, nonmetallic waste container.
* For large spills, call EH&S Chemical and Radioactive Waste Disposal group at 352-392-8400 for clean-up assistance.
* See [UF EHS Spill Response](https://www.ehs.ufl.edu/departments/research-safety-services/hazardous-waste-management/spill-response/#:~:text=Call%20EH&S%20Chemical%20and%20Radioactive%20Waste) for additional information.

Emergency Response (Spill & Accident Procedures) Cont.

**Needlesticks**

* Allow to bleed freely. If necessary, control bleeding by applying direct pressure with a sterile gauze or bandage.
* Immediately wash with copious quantities of soap and water.
  + If eyes or mucous membranes are exposed, irrigate the area for at least 15 minutes with water.
* Seek medical treatment.
* Report the incident to the PI/supervisor and Environmental Health and Safety (352) 392-1591 and submit an online Injury /Incident Report (<https://apps.ehs.ufl.edu/incidents/>).

**If an emergency occurs outside of normal work hours, contact the University Police Department at 352-392-1111 or call 911.**

**Emergency Contact Numbers:**

* Principal Investigator: xxx-xxx-xxxx
* Lab Manager: xxx-xxx-xxxx
* Poison Control Center: 800-222-1222
* Emergency: 911
* EH&S: 352-392-1591

**Physical Address on Campus:**

[Add your lab’s address here.]

References

* [[UF EHS Safety-Engineered Sharps Fact Sheet](https://webfiles.ehs.ufl.edu/Safety_Eng_Sharps.pdf#:~:text=What%20is%20a%20safety-engineered%20sharp%3F%20The%20U.S.%20Occupational,effectively%20reduces%20the%20risk%20of%20an%20exposure%20incident.%E2%80%9D)](https://webfiles.ehs.ufl.edu/Safety_Eng_Sharps.pdf#:~:text=What%20is%20a%20safety-engineered%20sharp%3F%20The%20U.S.%20Occupational,effectively%20reduces%20the%20risk%20of%20an%20exposure%20incident.%E2%80%9D)
* [UF EHS Spill Response](https://www.ehs.ufl.edu/departments/research-safety-services/hazardous-waste-management/spill-response/#:~:text=Call%20EH&S%20Chemical%20and%20Radioactive%20Waste)

Documents and attachments

List applicable forms and attachments here.